


Kali Lighting Quotation Sheet

Date：             Product：Emergency LED Exit Sign Plate     Model：
	Supplier: Foshan Kaili Lighting Technology Co., Ltd.
	Buyer:

	Add: No.3 building, Zhifu Park Industrial Town, Shunde, Foshan city; Guangdong Province, China (528300)
	Add：

	Contact：Steward
	Contact： 

	Mobile: 86 180 227 99159
	Mobile:

	E-mail: sales@kl-international.com
	E-mail：



	Light Box Parameter

	No.
	Item
	Parameter
	Remark

	1
	Surface Brightness
	________cd/m2
	International Standards: ≧100 cd/m2 

	2
	Color Temperature
	
	4000K / 6500K

	3
	Size (Box only) 
	L :
	Use mm as unit
If no specific size, will use general size.

	
	
	W :
	

	
	
	H :
	

	4
	Size (Box with Light)
	L :
	Use mm as unit

	
	
	W :
	

	5
	Installation
	☐Wall Mounted
☐Recessed Mounted
	

	Graphic Information

	6
	Front Plate Size
	L :
	- Use mm as unit
- If no specific size, will use general size.

	
	
	W :
	

	7
	Font / Pattern Size
	L :
	- Use mm as unit
- If there is no specific size, will adjust it according to the size of front plate

	
	
	W :
	

	8
	Pattern Requirement
	
	- Options available
- Please provide PDF




	Battery Parameter

	9
	* Main Voltage
	________V
	

	10
	* Discharge Duration
	________H
	

	11
	* Charging Time
	________H
	

	12
	Battery
	☐Ni-Cd
☐Ni-Mh
☐Lithium Iron Phosphate
	

	13
	Comply With EMC Standards
	☐Yes
☐No
	

	Other

	14
	Indicator Light
	☐Mains
☐Charging
☐Fault
	- Mains: Power on status is red.
- Charging: Charging status is red, fully charged is green.
- Fault: When a fault occurs, it turns yellow.

	15
	Button
	☐Text
	[image: 3981729748635_.pic]

	Quantity

	16
	Quantity
	
	

	Quotation

	17
	Price
	
	

	Product Reference

	[image: ][image: ][image: ][image: ]

	Remark

	- Asterisks are required.
- After the details are confirmed, we will provide a quotation reply as soon as possible.
- Process: Product Details → Sample Confirm → Order Confirm → Payment → Production.
- For all products, product samples will be made first, and then the samples will be sent to customers. production will start after order confirmed.
- The time required for production depends on factors such as product quantity, model, etc.
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Graphic   Information  
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